Hi, i'm Adrian Product specialist for RME Audio. In this Video we will take a quick look at the ARC USB, our brand new Remote Control for TotalMix FX.

The ARC USB is a powerful and freely assignable remote for complete control over TotalMix FX. It is the successor of the ARC MK1 and thanks to its new layout and vastly expanded hardware controls you get quick access to the most common functions of TotalMix FX and RME Interfaces.

The device itself comes in a nice sturdy metal case that matches the design of the UFX II and UFX+. 
By default the buttons correspond to their respective labels. This means that on the first two rows we can select between the different snapshots within TotalMix FX. On the third row, however, we can mono the main output, control the volumes of headphones 1 and 2 in combination with the encoder and listen to the external input if configured. 
The big encoder in the center of the unit controls the main volume.
On the lower part of the ARC USB we can engage the talkback mic, switch to a separate pair of speakers and dim the main output if desired.  

The ARC USB is designed to work seamlessly in every studio environment. The use of a bus powered USB1.1 connector allows cable lengths up to 10 meters with a standard USB2 cable. And the implemented class compliancy guarantees hassle free operation for Mac and PC systems without any drivers. On top of these great features the ARC USB is backwards compatible with all RME audio interfaces from 2001. 

In conjunction with the UFX+ and the UFX II the ARC USB also works as a standalone unit for handy control over DURec, Headphone Levels and Setups. We will show you these features in an upcoming in-depth video. 

With its small footprint, elegant design and driverless operation the ARC USB is a great addition for your studio.

So as you can see the ARC USB is the perfect companion for TotalMix FX and and RME Audio Interfaces. If you have any questions or ideas for future Videos. Please write them down in the comment section below. See you next Time on the RME Audio Channel.