Hey folks I'm Adrian product specialist for RME and in today's video i will show you how to set up two separate speaker pairs in TotalMix FX and how to control them with the ARC USB.

First we need to connect the RME Audio interface with the speakers and for this demo we use the Fireface 802. On the back we have 8 balanced line level outputs and outputs 1 & 2
will be for speaker A and outputs 3 & 4 will be for speaker B. where one is for the left speaker and two is for the right speaker and so on.

In TotalMix FX we go to the right hand corner and click on assign and we can then select the speakers, so the main out will be balanced outputs 1 & 2 and speaker B will go to outputs 3 & 4. As you can see now a new speaker popped up and we can control each volume separately. 

We can also link the speakers so they have the same level when we change one or another. With the ARC USB we can now remote control the speakers, so we can change the volume of both speakers. we can mono each speaker and we can dim each speaker and with a speaker B select we switch between speaker A and speaker B.