ADI-2 Pro
2-Channel high-end AD/DA Converter

RME’s Anniversary reference AD/DA converter is an USB 2.0 DAC, interface and a high-end headphone ­amplifier. Its design, unique specifications, user features and its ability to deliver crystal transparency, make it ­perfect for mastering and measurement applications as well as the ultimate tool for audiophiles everywhere.

The ADI-2 boasts high-grade components and intelligent circuitry throughout its half rack design. With RME’s fresh concept in Plug & Play the comprehensive feature set is easy to set up and use. Based on current connections the ADI-2 Pro will automatically switch to AD/DA converter, USB interface or analog preamp mode. A specific mode can be set if required.

The ADI-2 Pro includes two servo-balanced analog inputs on combo XLR/ TRS jacks, two separate balanced and unbalanced outputs on XLR and TRS, two stereo ‘Extreme Power’ headphone outputs on the front, an optical SPDIF I/O that also understands ADAT, plus coaxial SPDIF (RCA) and AES I/O (XLR) via an included breakout cable. This universal set of I/O options offers quality and flexible ­connectivity to those who take a no-compromise approach to audio. 

The ADI-2 Pro offers sample rates of up to 768kHz for both AD (2) and DA (4) channels of ­conversion.

Connectivity / Features
•	High-End AD/DA Conversion
•	1x Stereo Analog I/O
•	1x ADAT or SPDIF I/O
•	2x “Extreme Power“ Headphone Outputs
•	High-resolution IPS display
•	Auto Mode
•	1 x USB 2.0 (USB 3.0 compatible)
•	Optional: 19“ Rackmount Kit (RM19-X)
•	Optional: 19“ Rackmount (Unirack)

http://www.rme-audio.de/en/products/adi_2-pro.php

Suggested Keywords:
 RME Audio, AD/DA Converter, Pro-Audio